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 DATI TECNICI
Material: Fabric
Weight: 5,800 kg
Maximum production Industrial Coil and Chamine: (depends on the product to be cut) 20 cuts/minute.
Maximum production Industrial Hygiene: (depends on the product to be cut) 45 cuts/minute.
Installed power / Voltage: 12.5 Kw / 380 V.a.c.
Machine structure color: GREY RAL 7035.
Mudguard color: BLUE RAL 5024.
Machine/manual language Spanish.
CARATTERISTICHE
Disc roller advancement and cutting table.
Roll accumulator with stainless steel plate
Automatic accumulator input belt.
Ø810 and Ø1000 mm discs can be mounted
Installed power 12.5 Kw.
EEC regulations.
FORMATO Y DIMENSIONES
Width x Depth: 7,467 mm x 4260.50 mm
Height: 3,125 mm
ACCESSORI OPZIONALI
Available jaw sizes:
-	ø110 a ø130
-	ø150 a ø170
-	ø170 a ø200
-	ø200 a ø230
-	ø240 a ø270
-	ø260 a ø290
-	ø290 a ø320
-	ø320 a ø350
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[MAQUINA BASE

[anchura x Profundidad 7.467 mm 426050

[Altura 3125
peso 5800 kg |
Material Tissue |

Produccién maxima Bobina industral 10 cortes / minuto)

(depende det producto a cortar)

Produccién maxima Higiénico industrial: 45 cortes/minuto

(depende det producto a cortar)

Potencia instalada / Voltaje: 125 Kw/ 380 Yica |
|Color de Ia estructura de 2 maquina: GRIS RAL 7035
|Color de las defensas: AZULRAL 5024
dioma de 1a maquina / manual a especificar |
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